On windows, Install python2.7

C:\Python27\python.exe -m pip install --upgrade pip

C:\Python27\python -m pip install pyserial

C:\Python27\python.exe .\Gen2Test.py -port=COM5

Sending inventory cmd

Found 1 Gen2 brds.

Addr = ['0x20']

0x20 WingCfg = 0x02020202

0x20 W[0]:INP\_WING, W[1]:INP\_WING, W[2]:INP\_WING, W[3]:INP\_WING

C:\pinball-maker\open-pinball-project-code\Python\Gen2Test> C:\Python27\python.exe .\Gen2Test.py -port=COM5 -saveCfg -loadCfg=STM32card1.py

Sending inventory cmd

Found 1 Gen2 brds.

Addr = ['0x20']

0x20 WingCfg = 0x01010202

0x20 W[0]:SOL\_WING, W[1]:SOL\_WING, W[2]:INP\_WING, W[3]:INP\_WING

loadFileName = STM32card1

Sending wing cfg.

Sending input cfg.

Sending solenoid cfg.

Sending color table cfg.

Sending save cfg command.

Done save cfg command.

C:\pinball-maker\open-pinball-project-code\Python\Gen2Test> C:\Python27\python.exe .\Gen2Test.py -port=COM5

Sending inventory cmd

Found 1 Gen2 brds.

Addr = ['0x20']

0x20 WingCfg = 0x06010102

0x20 W[0]:NEO\_WING, W[1]:SOL\_WING, W[2]:SOL\_WING, W[3]:INP\_WING

C:\Python27\python.exe .\Gen2Test.py -port=COM5 -ser=5

Set Serial